# Rainmaker Display (rev001)

1. Entering Bootloader
2. Update Instructions
3. Changelog

## Entering Bootloader

1. Turn off power to your modular system.
2. Remove the module from your modular case.
3. Connect a micro-USB cable from the USB port on the top edge of the display to your computer.
4. Hold down the tiny button on the edge of the display board while powering on your modular system. See the highlighted green circle in the image above for the exact location.

## Update Instructions

1. From the version menu above, select the firmware version you will be updating to.
2. Click the Update button in the bottom of this window. You will see the progress of the update in the log window and your module may begin to flash. You will see an “Update completed successfully” message at the end of the update.
3. Turn your modular off and back on again, you're now ready to use your updated module.
4. If there are any problems please contact us via the Help button on our website. Be sure to include the full log window output, the firmware updater version downloaded, and the OS you are using.

## Changelog

### 1.09 (2019-04-25)

- Update for FPGA revision 143 (2019-11-04)

### 1.07 (2017-10-04)

- Update for FPGA revision 8

### 1.04 (2017-01-30)

- Update for FPGA revision 6

### 1.02 (2016-05-11)

- Fix order of clear buffer and toggle ping-pong items in the trigger menu.

### 1.01 (2016-04-27)

- Initial release