# Sealegs

1. Entering Bootloader
2. Update Instructions
3. Changelog

## Entering Bootloader

1. Turn off power to your modular system.
2. Connect a USB cable from the rear of the module to your computer.
3. Hold down the BOOT button on the rear of the module and turn on power to your modular system.

## Update Instructions

1. From the version menu above, select the firmware version you will be updating to.
2. Click the Update button in the bottom of this window. You will see the progress of the update in the log window and your module may begin to flash. You will see an “Update completed successfully” message at the end of the update.
3. Turn your modular off and back on again, you're now ready to use your updated module.
4. If there are any problems please contact us via the Help button on our website. Be sure to include the full log window output, the firmware updater version downloaded, and the OS you are using.

## Changelog

### 1.2.2.0 (2025-04-15)

- Fixed: Mod would reset to W&F on boot, it now matches knob position on boot.

### 1.2.1.0

- Minor bug fixes and tuning.

### 1.2.0.0

- Tweaks: Gain Staging updates — This update reduces the attenuation on signals passing through Sealegs; as a result, the MIX (wet/dry) control is much more balanced and the overall output of the module is louder, matching closer to your input. Adjust your mixes accordingly.
- Tweak: Wider "Detent" for setting input trim to 1x (Noon).
- New: Send/Return Mode (Hold DELAY SYNC on boot) —
  - A special mode intended to be used on an Aux Send from a mixer.
  - DRY signal is NOT passed through.
  - MIX controls the WET level only.

### 1.1.1.0

- Tweak: Tighter timing when frozen in all 3 models, both synced and unsynced.
- Other: Minor tweaks and tuning.

### 1.1.0.0

- Tweak: Freeze is now "clickless" on all modes.
  - Notes about freeze: Tape and BBD emulate an analog style freeze (ie. cutting the input to delay and locking feedback at 100%), they will both absorb modulation and time changes into the frozen audio. Specifically in BBD mode, you may find accumulating signal/frequency loss when freezing by nature of emulating an analog BBD with limited sample rate, especially at longer times. Tape mode will hold its audio level much better, while slowly saturating as a tape delay would. Digital mode actually freezes the audio buffer, and will maintain it's contents indefinitely, and will not be modified by modulation or time changes.
- New: Flexible Drive Signal Path —
  - Hold ALT and Move the FOG POS switch to set.
  - Setting will be saved across reboots.
  - See updated manual for full details on the new routing options.
  - IN = Original Drive Functionality. (Default)
  - DLY = Drive is bypassed on the Dry signal, and only passed into the Delay.
  - MIX = Drive is end-of-chain POST MIX.
- Other: Misc tweaks and tuning.
- Updated manual available at intellijel.com/support.

### 1.0.0.4/5

- Initial release.