# µMIDI

1. Entering Bootloader
2. Update Instructions
3. Changelog

## Entering Bootloader

1. Turn off power to your modular system.
2. Disconnect all cables, including patch cables and DIN MIDI cables from the µMIDI.
3. Connect a USB cable from the µMIDI module to your computer.
4. Hold down the LEARN button on the module and turn on power to your modular system.

## Update Instructions

1. From the version menu above, select the firmware version you will be updating to.
2. Click the Update button in the bottom of this window. You will see the progress of the update in the log window and your module may begin to flash. You will see an “Update completed successfully” message at the end of the update.
3. Turn your modular off and back on again, you're now ready to use your updated module.
4. If there are any problems please contact us via the Help button on our website. Be sure to include the full log window output, the firmware updater version downloaded, and the OS you are using.

## Changelog

### 1.15 (2017-05-11)

- Fix some settings not saving.

### 1.14 (2016-09-22)

- Add option to disable clock outputs when sequencer is not running.
- Allow option for CC output to respond to channel aftertouch.

### 1.13 (2016-06-22)

- Fix USB communication problem on some Windows machines.

### 1.12 (2016-06-06)

- Fix stuck gate when using last note priority.

### 1.11 (2016-05-25)

- Ability to set coarse and fine tuning via RPN messages. The new default tuning is -24 so that 0V corresponds to C0 in Ableton Live.
- Send reset signal slightly before clock
- Fix saving of settings
- Compatibility with the new online configuration utility

### 1.00 (2015-12-04)

- Initial release.