# Steppy 1U (rev003) and 3U (rev002)

1. Entering Bootloader
2. Update Instructions
3. Changelog

## Entering Bootloader

1. Turn off power to your modular system.
2. Connect a USB cable from the rear of the module to your computer.
3. Hold down the EDIT (Red) button and turn on power to your modular system.

## Update Instructions

1. From the version menu above, select the firmware version you will be updating to.
2. Click the Update button in the bottom of this window. You will see the progress of the update in the log window and your module may begin to flash. You will see an “Update completed successfully” message at the end of the update.
3. Turn your modular off and back on again, you're now ready to use your updated module.
4. If there are any problems please contact us via the Help button on our website. Be sure to include the full log window output, the firmware updater version downloaded, and the OS you are using.

## Changelog

### 1.2.3.0 (2022-09-20)

- TWEAK: Changed handling of gate timing on the first pulse after the clock has been stopped. (Will prevent a really long gate when the sequence starts.)
- TWEAK: Reset sequencer to step 1 on regular preset load.

### 1.2.2.1 (2021-12-17)

- Support for rev003 hardware.

### 1.2.1 (2020-01-17)

- FIXED: Hanging after upgrade to 1.2.0

### 1.2.0 (2020-01-16)

- NEW: Latching Loopy mode. When Holding down Loopy steps, tap the SEL button to Latch your loop. Press a step button to release. If you change your Loopy steps, you will need to press SEL to latch them again.
- NEW: Delayed load. When on the LOAD page, you can long-press a preset to have it load when the current pattern reaches its last step on track 1.
- NEW: Muted tap entry mode. When in TAP Recording Mode, you can press the "PROB" button to toggle muting your taps. The ABCD buttons will turn Yellow to indicate Muted.
- NEW: Step Edit mode (per-step gate length, delay, probability (and still Ratchets). This changes the UI for editing ratchets, as you can now edit 3 other parameters. Details will be found the updated manual.
- FIXED: Track Probability is now applied to the current position, and will not randomize individual ratchets.

### 1.11 (2019-10-10)

- Additional filtering on Clock input to handle imprecise clock pulses.

### 1.10 (2019-08-14)

- Added toggle for RESET Mode and New RUN Mode — Hold RST (Save) on boot.
- On the SEL page, you'll see the RST LED Lit solid Yellow if RUN mode is enabled.

### 1.00 (2018-10-15)

- Initial release.